**Hinged Coat Rack Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install custom length wall mounted coat rack.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking for coat racks.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: HCR unit by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS:
	1. Brackets are solid cast aluminum powder coated black.
	2. Shelf slat is extruded aluminum (specify finish either silver or bronze) or hardwood slat (specify type walnut, light oak, medium oak, or unfinished oak).
	3. Hanger bar shall be 1" black aluminum tube capped at each end.
	4. Accessories: EMCO ball top hanger (specify hanger type) and “A” receptacle shall be spaced 4 per foot.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
	2. Install bracket using “fasteners by others” appropriate for wall type.
	3. The bracket height shall be based upon architect’s specified shelf height.
	4. Install slat and rod using EMCO fasteners.
	5. Wipe down shelves to remove dust.
	6. Remove all trash and debris.