**Garment Hook Panel Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install wall mounted hook panels.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: GHP series hook panel by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS: Panel shall be of solid (walnut or oak) 5/8”x 5 5/8”x 6” hardwood and drilled for one hook. The finish is to be (specify walnut, medium oak, light oak, or unfinished oak).
3. GHP panels shall have one P1 hook (specify finish either silver or black) centered on panel. All hooks to be installed at the factory.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
  2. Predrill panel to accommodate wall fasteners.
  3. Fasteners shall be recessed to allow wood buttons to be installed to cover screw heads.
  4. Check to make sure pane is level.
  5. Attach panel to wall.
  6. Wipe down panel to remove dust.
  7. Remove all trash and debris.