**R2 Coat Rack Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install custom length wall mounted coat rack.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking for coat racks.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: R2 unit by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS:
	1. Wall strips are 1/2" extruded aluminum 24” long, powder coated black.
	2. Brackets are solid cast aluminum powder coated black. Bracket screws are included to allow for height adjustment.
	3. Shelf slat is extruded aluminum (specify finish either silver or bronze) or hardwood slat (specify type walnut, light oak, medium oak, or unfinished oak).
	4. Hanger bar shall be 1" black aluminum tube capped at each end.
	5. Accessories: EMCO hangers (specify any model EMCO hanger and, if required, receptacles) shall be spaced 4 per foot.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
	2. Install wall strip using “fasteners by others” appropriate for wall type.
	3. The wall strip height shall be based upon architect’s specified height for shelf.
	4. Install brackets in wall strip using EMCO fasteners.
	5. Install slat and rod using EMCO fasteners.
	6. Wipe down shelves to remove dust.
	7. Remove all trash and debris.