**S10 Hook Specifications**

**PART 1 - GENERAL**

1. DESCRIPTION: Furnish and install wall mounted hooks.
2. RELATED WORK: (Refer to Section of Specs which applies to wall blocking.)

**PART 2 - PRODUCTS**

1. MANUFACTURER: S10 hook by EMCO Specialty Products, Inc., Kansas City, KS.
2. MATERIALS: Hook shall be of solid steel 5 5/8” high, 3/4” wide and projecting 3 3/8” from the wall. The finish is to be powder coated. Color to be black.

**PART 3 - EXECUTION**

INSTALLATION:

* 1. Install wall blocking.
  2. Install hook using manufacturer’s fasteners if appropriate for wall type. (Screws provided by EMCO are not intended for all wall types.)
  3. Install hook at height & location specified by architect.
  4. Wipe down hook to remove dust.
  5. Remove all trash and debris.